
Sound Blaster 16 ISA driver for Minix 3

Note: supports audio playback and volume control (mixer),
recording is not yet supported


Installation instructions SB16 driver Minix >= 3.0.7

- set IRQ and I/O address in sb16.h
(default 7 and 220)
- make install
- MAKEDEV /dev/audio (if /dev/audio doesn't allready exist)
- service up /usr/sbin/sb16_dsp -dev /dev/audio
- service up /usr/sbin/sb16_mixer -dev /dev/mixer
done... (you can include the last 2 lines in /usr/etc/rc)


Peter Boonstoppel - September 2005
paboonst@cs.vu.nl

